**Life cycle assessment of Power-to-Methane systems with CO2 supplied by Chemical Looping Combustion of biomass**

Alberto Navajas1,2, Teresa Mendiara3\*, Luis M. Gandía1,2, Alberto Abad3, Francisco García-Labiano3, Luis F. de Diego3

1 Department of Science, Public University of Navarre, Arrosadía Campus s/n, E-31006 Pamplona, Spain

2 Institute for Advanced Materials and Mathematics (InaMat2), Public University of Navarre, Arrosadía Campus s/n, E-31006 Pamplona, Spain

3 Department of Energy and Environment, Instituto de Carboquímica-ICB-CSIC

Miguel Luesma Castán 4, 50018, Zaragoza, Spain.

\* Corresponding author: tmendiara@icb.csic.es

Phone: + 34 976 733 977;

Fax: +34 976 733 318

**Table S1**. Environmental impact indicators, LCIA method used for their calculation, and units of the indicator

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Environmental Impact Indicator** | **Abbreviation** | **Calculation Method** | **Unit** | **Classification** |
| Global Warming Potential | GWP | IPPC2007 [1] | kg CO2 Eq. | I |
| Ozone Depletion Potential | ODP | WMO1999 [2] | kg CFC-11 Eq. | I |
| Respiratory Inorganics | RI | UNEP [3] | kg PM2,5 Eq. | I |
| Ionising radiation | IR | ReCiPe2008 [4] | kg U235 Eq. | II |
| Photochemical ozone formation | POF | ReCiPe 2008 [5] | kg NMVOC Eq. | II |
| Acidification Potential | AC | [6, 7] | Mole of H+ Eq. | II |
| Terrestial Eutrophication | EUT | [6, 7] | Mole f N Eq. | II |
| Aquatic freshwater Eutrophication | EUF | ReCiPe2008 [8] | kg of N Eq. | II |
| Aquatic marine Eutrophication | EUM | ReCiPe2008 [8] | kg of N Eq. | II |
| Human Toxicity Potential, Cancer effects | HTC | UseTox [9] | Comparative Toxic Unit for Human Health (CTUh) | II/III |
| Human Toxicity Potential, Non Cancer Effects | HTNC | UseTox [9] | CTUh | II/III |
| Ecotoxicity freshwater | ECFW | UseTox [9] | Comparative Toxic Unit for ecosystems (CTUe) | II/III |
| Resource Use Minerals and Metals | RUM | ADP [10]  | kg Sb Eq. | III |
| Water Use – Water Scarcity | WU | UNEP [11]  | m3 Eq. | III |
| Land Use | LU | LANCA [12]  | Soil Quality Index | III |
| Resource Use Energy Carriers | RUE | ADP [10]  | MJ | III |

**Table S2**. Values for the environmental impact indicators LCIA obtained for the different PtM-bioCLC schemes

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **iG-CLC\_mOC** |  | **iG-CLC\_sOC** |  | **CLOU** |  | **Base Case** |
|  | **NOx** | **no NOx** | **NOx** | **no NOx** | **NOx** | **no NOx** |  |
| **GWP** | -1,05E+09 | -1,05E+09 | -1,06E+09 | -1,06E+09 | -8,62E+08 | -8,62E+08 | 2,62E+08 |
| **ODP** | 3,33E-04 | 3,33E-04 | 3,33E-04 | 3,33E-04 | 3,33E-04 | 3,33E-04 | 3,33E-04 |
| **RI** | 2,14E+01 | 5,52E-01 | 2,14E+01 | 5,69E-01 | 1,86E+01 | 4,94E-01 | 8,40E+00 |
| **IR** | 8,68E+06 | 8,68E+06 | 8,66E+06 | 8,66E+06 | 8,66E+06 | 8,66E+06 | 8,82E+06 |
| **POF** | 1,29E+07 | -7,36E+04 | 1,30E+07 | -4,92E+04 | 1,12E+07 | -8,36E+04 | 6,77E+05 |
| **AC** | 9,71E+06 | 7,63E+04 | 9,72E+06 | 9,42E+04 | 8,45E+06 | 7,24E+04 | 7,18E+05 |
| **EUT** | 5,50E+07 | -4,85E+05 | 5,51E+07 | -3,80E+05 | 4,77E+07 | -5,02E+05 | 2,19E+06 |
| **EUF** | 2,80E+02 | 2,80E+02 | 2,80E+02 | 2,80E+02 | 2,73E+02 | 2,73E+02 | 2,53E+02 |
| **EUM** | 5,02E+06 | -4,41E+04 | 5,03E+06 | -3,45E+04 | 4,36E+06 | -4,55E+04 | 2,01E+05 |
| **HTC** | 4,13E-01 | 4,13E-01 | 4,13E-01 | 4,13E-01 | 4,12E-01 | 4,12E-01 | 4,15E-01 |
| **HTNC** | 4,71E+00 | 4,71E+00 | 4,70E+00 | 4,70E+00 | 4,65E+00 | 4,65E+00 | 5,58E+00 |
| **ECFW** | 6,13E+08 | 6,13E+08 | 6,09E+08 | 6,09E+08 | 5,86E+08 | 5,86E+08 | 7,48E+08 |
| **LU** | 2,59E+10 | 2,59E+10 | 2,59E+10 | 2,59E+10 | 2,27E+10 | 2,27E+10 | 5,72E+08 |
| **WU** | 2,62E+09 | 2,62E+09 | 2,62E+09 | 2,62E+09 | 2,62E+09 | 2,62E+09 | 2,62E+09 |
| **RUE** | -8,54E+09 | -8,54E+09 | -8,57E+09 | -8,57E+09 | -8,62E+09 | -8,62E+09 | 1,16E+10 |
| **RUM** | 2,96E+03 | 2,96E+03 | 2,98E+03 | 2,98E+03 | 3,03E+03 | 3,03E+03 | 3,01E+03 |

**References**

[1] IPCC, Anthropogenic and Natural Radiative Forcing. In Climate Change 2013: The Physical Science Basis: Working Group I Contribution to the Fifth Assessment Report of the Intergovernmental Panel on Climate Change, in: C.U. Press (Ed.) New York, 2014, pp. 659-740.

[2] WMO, Global Ozone Research and Monitoring Project - Report No. 44, Geneva, 1998.

[3] P. Fantke, O. Jolliet, J.S. Evans, J.S. Apte, A.J. Cohen, O.O. Hanninen, F. Hurley, M.J. Jantunen, M. Jerrett, J.I. Levy, M.M. Loh, J.D. Marshall, B.G. Miller, P. Preiss, J.V. Spadaro, M. Tainio, J.T. Tuomisto, C.J. Weschler, T.E. McKone, Health effects of fine particulate matter in life cycle impact assessment: findings from the Basel Guidance Workshop, International Journal of Life Cycle Assessment 20(2) (2015) 276-288.

[4] R. Frischknecht, A. Braunschweig, P. Hofstetter, P. Suter, Human health damages due to ionising radiation in life cycle impact assessment, Environmental Impact Assessment Review 20(2) (2000) 159-189.

[5] R. van Zelm, M.A.J. Huijbregts, H.A. den Hollander, H.A. van Jaarsveld, F.J. Sauter, J. Struijs, H.J. van Wijnen, D. van de Meent, European characterization factors for human health damage of PM10 and ozone in life cycle impact assessment, Atmos. Environ. 42(3) (2008) 441-453.

[6] J. Seppälä, M. Posch, M. Johansson, J.P. Hettelingh, Country-dependent characterisation factors for acidification and terrestrial eutrophication based on accumulated exceedance as an impact category indicator, International Journal of Life Cycle Assessment 11(6) (2006) 403-416.

[7] M. Posch, J. Seppälä, J.P. Hettelingh, M. Johansson, M. Margni, O. Jolliet, The role of atmospheric dispersion models and ecosystem sensitivity in the determination of characterisation factors for acidifying and eutrophying emissions in LCIA, International Journal of Life Cycle Assessment 13(6) (2008) 477-486.

[8] M. Goedkoop, R. Heijungs, M. Huijbregts, A. De Schryver, J. Struijs, R. van Zelm, ReCiPe 2008. A life cycle impact assessment method which comprises harmonised category indicators at the midpoint and the endpoint level in: S.P.a.E. Ministry of Housing (Ed.) The Netherlands, 2009.

[9] R.K. Rosenbaum, T.M. Bachmann, L.S. Gold, M.A.J. Huijbregts, O. Jolliet, R. Juraske, A. Koehler, H.F. Larsen, M. MacLeod, M. Margni, T.E. McKone, J. Payet, M. Schuhmacher, D. Van De Meent, M.Z. Hauschild, USEtox - The UNEP-SETAC toxicity model: Recommended characterisation factors for human toxicity and freshwater ecotoxicity in life cycle impact assessment, International Journal of Life Cycle Assessment 13(7) (2008) 532-546.

[10] L. van Oers, A. de Koning, J.B. Guinée, G. Huppes, Abiotic resource depletion in LCA, 2002.

[11] A.M. Boulay, J. Bare, L. Benini, M. Berger, M.J. Lathuilliere, A. Manzardo, M. Margni, M. Motoshita, M. Nunez, A.V. Pastor, B. Ridoutt, T. Oki, S. Worbe, S. Pfister, The WULCA consensus characterization model for water scarcity footprints: assessing impacts of water consumption based on available water remaining (AWARE), International Journal of Life Cycle Assessment 23(2) (2018) 368-378.

[12] U. Bos, R. Horn, T. Beck, J.P. Lindner, M. Fischer, LANCA® Characterization Factors for  Life Cycle Impact Assessment Version 2.0 2016, p. 166.